(footprint "Choc_v1_17x17mm_spacing"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "SW13"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "5b8b2509-cc48-47a4-8fce-ab86fcffde68")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "SW_SPST"
		(at 0 0 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "aacfd6f5-65b7-4133-8281-45c322585029")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "~"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "2a52bd72-0c3f-48f2-a724-e8d669cfe14f")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Choc v1 keyswitch"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "60fcfa86-dd34-4fec-98c7-ae7cfcb9d8ee")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "JLCPCB Part Number" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7c202ef6-551b-4cdd-9ae7-26d21269315b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole exclude_from_bom)
	(fp_line
		(start -8.5 -8.5)
		(end 8.5 -8.5)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "Dwgs.User")
		(uuid "7699333a-f4db-4625-a04f-ceb94bcace22")
	)
	(fp_line
		(start -8.5 8.5)
		(end -8.5 -8.5)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "Dwgs.User")
		(uuid "84e98009-a36c-4a17-a569-fde4fbea482e")
	)
	(fp_line
		(start -7 -6)
		(end -7 -7)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "Dwgs.User")
		(uuid "c3e13b08-e233-4954-86c1-a796d408a520")
	)
	(fp_line
		(start -7 7)
		(end -7 6)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "Dwgs.User")
		(uuid "d1e7dd04-eabb-4c9c-9bd8-3860764a3590")
	)
	(fp_line
		(start -7 7)
		(end -6 7)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "Dwgs.User")
		(uuid "49c30273-bb99-474a-8452-3e95b3920c2c")
	)
	(fp_line
		(start -6 -7)
		(end -7 -7)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "Dwgs.User")
		(uuid "54c7fd19-7ce7-4c39-9f25-859237f52ffc")
	)
	(fp_line
		(start 6 7)
		(end 7 7)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "Dwgs.User")
		(uuid "ede29a3f-a9a6-47df-836d-c4772ed880b1")
	)
	(fp_line
		(start 7 -7)
		(end 6 -7)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "Dwgs.User")
		(uuid "65ba7540-2b09-40be-8697-21853845d68e")
	)
	(fp_line
		(start 7 -7)
		(end 7 -6)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "Dwgs.User")
		(uuid "f1d0021a-165e-4889-aa81-e278d0d78cc6")
	)
	(fp_line
		(start 7 6)
		(end 7 7)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "Dwgs.User")
		(uuid "c89ad502-74fd-4515-831a-e77ed3111cbc")
	)
	(fp_line
		(start 8.5 -8.5)
		(end 8.5 8.5)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "Dwgs.User")
		(uuid "8210335c-d6a0-4308-8c53-57e96bf7ef0e")
	)
	(fp_line
		(start 8.5 8.5)
		(end -8.5 8.5)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "Dwgs.User")
		(uuid "36a01b58-12db-413b-bdf4-8e7e60f5b51e")
	)
	(pad "" np_thru_hole circle
		(at -5.5 0 180)
		(size 1.7018 1.7018)
		(drill 1.7018)
		(layers "*.Cu" "*.Mask")
		(uuid "5add7edf-3b4d-49b6-9b81-fda7ac714069")
	)
	(pad "" np_thru_hole circle
		(at 0 0 180)
		(size 3.429 3.429)
		(drill 3.429)
		(layers "*.Cu" "*.Mask")
		(uuid "42fb6c34-34c0-481b-8207-70ca722ad0fb")
	)
	(pad "" np_thru_hole circle
		(at 5.5 0 180)
		(size 1.7018 1.7018)
		(drill 1.7018)
		(layers "*.Cu" "*.Mask")
		(uuid "cb8a715d-8e12-4712-82bb-413e7d72aaf4")
	)
	(pad "1" thru_hole circle
		(at -5 3.8 180)
		(size 2.032 2.032)
		(drill 1.27)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6ef19e7b-3b30-4e26-bfe0-826067df6d4a")
	)
	(pad "2" thru_hole circle
		(at 0 5.9 180)
		(size 2.032 2.032)
		(drill 1.27)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5b307a43-4634-436d-b54b-63eed3a5e24c")
	)
	(embedded_fonts no)
)
