(footprint "diode_ref"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SOD-123")
	(tags "SOD-123")
	(property "Reference" "REF**"
		(at 0 -2 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "01e8053f-44d8-4376-a89b-9f588e2692f8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Val**"
		(at 0 2.1 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "d3e6363d-570b-499b-bd14-85c236f50f1c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "19d9da19-3d2f-41cb-b101-4ebb2852f8dd")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "509b0d62-1491-4be6-8733-0bc82a0fe79f")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Device" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a5b3124a-3976-4dde-a579-e44e60d66859")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Sim.Pins" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7ba2fb48-1935-44df-b712-47d8450caf22")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr board_only exclude_from_pos_files exclude_from_bom allow_missing_courtyard
		dnp
	)
	(fp_line
		(start -2.36 -1)
		(end -2.36 1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "f1ee7def-c87f-4390-85da-384fa416f027")
	)
	(fp_line
		(start -2.36 -1)
		(end 1.65 -1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5be1ad38-498d-4614-ab33-1f5fca831a1c")
	)
	(fp_line
		(start -2.36 1)
		(end 1.65 1)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2a226bcc-c328-4bb0-988f-a0adb2170048")
	)
	(fp_line
		(start -1.5 0)
		(end -0.35 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "1e85836c-c7c6-4a85-ba61-d94a2380b711")
	)
	(fp_line
		(start -0.35 0)
		(end -0.35 -0.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "717d53d8-692f-40d6-b06d-5d6c36b24121")
	)
	(fp_line
		(start -0.35 0)
		(end -0.35 0.55)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2bd7d3a5-cdef-4956-8b5d-b0ee139311b4")
	)
	(fp_line
		(start -0.35 0)
		(end 0.25 -0.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "3badc5bf-0ca6-40b6-a100-dc471ddd4000")
	)
	(fp_line
		(start 0.25 -0.4)
		(end 0.25 0.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "fdb3ee29-8d08-406a-a150-9def21d52a22")
	)
	(fp_line
		(start 0.25 0)
		(end 1.5 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4015e3de-4a9f-40f7-8485-bd84f67a6dc3")
	)
	(fp_line
		(start 0.25 0.4)
		(end -0.35 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c1d435cf-46cb-445c-bf47-bccc8505c1e9")
	)
	(fp_text user "Diode Ref"
		(at 0 -1.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "463e2f17-b8e7-4983-8651-0eccb798eb46")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify bottom)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
